#N canvas 168 84 1037 596 10;
#X obj 102 511 dac~;
#X msg 115 354 bang;
#X obj 66 290 metro 400;
#X obj 66 269 tgl 15 0 empty empty empty 17 7 0 10 -262144 -1 -1 0
1;
#X obj 115 377 perk-clap;
#X msg 276 198 0 \$1;
#X msg 209 105 0.1 1000;
#X msg 294 107 -0.1 1000;
#X msg 380 276 1 1000;
#X msg 268 105 0;
#X msg 322 278 0.5 1000;
#X obj 276 167 line 0 20;
#X obj 322 311 line 1 20;
#X msg 323 336 6 \$1;
#X text 362 336 muliply slider 6 by amount \$1;
#X text 317 197 add amount \$1 to slider 0;
#X msg 127 210 1 \$1;
#X text 229 79 ADDITION MODULATION;
#X text 322 252 MULTIPLICATION MODULATION;
#X floatatom 124 158 5 0 100 0 - - -;
#X obj 125 184 / 100;
#X text 121 136 SET CONTROL;
#X text 167 214 set slider 1;
#X text 168 232 to value \$1;
#X msg 599 144 1;
#X msg 630 143 0;
#X obj 629 122 delay 200;
#X obj 600 178 s \$0-note;
#X obj 600 95 t b b;
#X obj 597 71 metro 400;
#X obj 597 50 tgl 15 0 empty empty empty 17 7 0 10 -262144 -1 -1 0
1;
#X obj 559 0 cnv 15 1 500 empty empty empty 20 12 0 14 -233017 -66577
0;
#X text 578 -3 MODULATION BY ADSR / LFO INPUT;
#X text 38 -8 DIY synth voices \, percussion \, and effects can have
their parameters modulated by external input. the inlets for this are
1) set control 2) add to control value 3) multiply control value. modulation
can be achieved by sending values directly to the inlets \, or using
the DIY adsr/lfo modules.;
#X obj 697 513 dac~;
#X obj 753 426 eee-adsr~;
#X obj 700 469 *~;
#X obj 601 306 syn-ugurphase;
#X obj 753 402 r \$0-note;
#X obj 714 176 eee-adsr;
#X msg 716 280 1 \$1;
#X obj 712 150 r \$0-note;
#X obj 600 283 mtof;
#X floatatom 599 263 5 0 0 0 - - -;
#X msg 598 243 35;
#X obj 597 221 loadbang;
#X obj 833 247 eee-lfo;
#X obj 718 256 +;
#X obj 834 342 t b f;
#X text 307 488 important note:;
#X text 314 506 if a modulation source is used \, and then the cable
to that source is disconnected \, the modulation value will remain
stored. after disconnecting a modulation source \, send message with
the number of the slider \, and a value of 0 to the addition inlet
\, or 1 to the multiplication inlet \, to restore the modulation to
zero.;
#X connect 1 0 4 0;
#X connect 2 0 1 0;
#X connect 3 0 2 0;
#X connect 4 0 0 0;
#X connect 4 0 0 1;
#X connect 5 0 4 2;
#X connect 6 0 11 0;
#X connect 7 0 11 0;
#X connect 8 0 12 0;
#X connect 9 0 11 0;
#X connect 10 0 12 0;
#X connect 11 0 5 0;
#X connect 12 0 13 0;
#X connect 13 0 4 3;
#X connect 16 0 4 1;
#X connect 19 0 20 0;
#X connect 20 0 16 0;
#X connect 24 0 27 0;
#X connect 25 0 27 0;
#X connect 26 0 25 0;
#X connect 28 0 24 0;
#X connect 28 1 26 0;
#X connect 29 0 28 0;
#X connect 30 0 29 0;
#X connect 35 0 36 1;
#X connect 36 0 34 0;
#X connect 36 0 34 1;
#X connect 37 0 36 0;
#X connect 38 0 35 0;
#X connect 39 0 47 0;
#X connect 40 0 37 2;
#X connect 41 0 39 0;
#X connect 42 0 37 0;
#X connect 43 0 42 0;
#X connect 44 0 43 0;
#X connect 45 0 44 0;
#X connect 46 0 48 0;
#X connect 47 0 40 0;
#X connect 48 0 47 0;
#X connect 48 1 47 1;
